
**Mercedes-Benz X-Class 2017-2020**

**Load-Lid Central Locking Fitting Instructions**

Thank you for purchasing a quality Utemaster™ product, our aim is providing you with as much assistance as possible throughout the fitting process. Please call 0800 683 352 or email: [sales@utemaster.co.nz](mailto:sales@utemaster.co.nz) if assistance is needed.

**We recommend watching the installation video before attempting to install**

Enter this address into your web browser to view the fitting video:  
**https://wi.st/33JZ47T**




**DESPATCH:**

1x 80606-26 / WHUTELL-08EXT 1.0

Diagram

Description automatically generated

**Step 1)** Under the passenger’s side rear wheel arch, remove the 4x clips indicated below and remove the plastic cover to expose the wires inside




**Step 2)** Open up the plastic sleeve around the wiring – wires inside should be green and grey




**Step 3)** Place one of the provided white clips over the grey wire



**Step 4)** Take the provided wiring loom and insert the black wire into the white clip



**Step 5)** Squeeze the metal clip with pliers until it sits completely inside the plastic clip



**Step 6)** Close the clip



**Step 7)** Repeat steps 3-6 for the green wire

*Black > Grey*

*White > Green*

**Step 8)** Insulation tape around both clips and the wire junction



**Step 9)** Feed the plug end of the wiring loom over the fuel filler and up to the front corner of the wellside



**Step 10)** Pull the plug through the hole in the front of the wellside and place it inside the wellside. Cable tie any slack cable remaining inside the wheel arch

**Step 11)** Reinstall the plastic cap



**Step 12)** Install the Load-Lid as per fitting instructions provided

**Step 13)** Connect the vehicle wiring loom to the plug already installed in the Load-Lid



Your central locking is now fully fitted and ready to use.

Thank you again for using Utemaster™ and don’t forget to keep checking our website for our latest innovations!